

**Fitting for wooden or glass folding sliding walls up to 120 kg (264 lbs.), with surface mounted**

**running track. Ceiling mounting. Fully opening.**

**Product-Highlights**

**Aesthetics**

Fitting for dividing rooms

**Flexibility**

Special running gear available as a supplement for fire protection

doors

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. opening width Height adjustable Soft close

Door material

Finish color of visible profiles

120 kg (264 lbs.)

42–80 mm (1 21/32'' to 3 5/32'')

4000 mm (13' 1 15/32'')

1000 mm (3' 3 3/8'')

7000 mm (22' 11 19/32'')

+/- 2 mm (3/32'')

No

Wood;Wood Glass Mix Stainless steel

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

120

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa 20 C Folding wall 120 consisting of double running track (stainless steel), running gear with 4 steel ball bearings, steel running gear suspension profile, top pivot bearing, bottom guide bracket, bottom guide track, ball bearing hinge, pin lock.

Optional:

(….) Espagnolette lock with rotary handle or detachable key (….) Running gear for fire protection sliding doors

# Interfaces Door leaf

* Recess for top suspension profile (H × W) 32 × 32 mm (1 1/4'' x 1 1/4'')
* Recess for bracket at side (W × D) 32 × 8 mm (1 1/4'' x 5/16'')
* Screw fixing of the suspension profiles
* Recess for bottom guide profile at side and bottom (W × D) 32 × 8 mm (1 1/4'' x 5/16'')

# Floor guide

* embedded in floor

# Hawa Sliding Solutions AG

Untere Fischbachstrasse 4, 8932 Mettmenstetten, Switzerland

Phone +41 44 787 17 17, [info@hawa.com,](mailto:info@hawa.com) [www.hawa.com](http://www.hawa.com/) 1