

**Fitting for top-running wooden doors up to 40 kg (88 lbs.), with screwed on running track.**

**Design Inslide. Fully opening.**

**Product-Highlights**

**Flexibility**

Curved tracks with a radius of more than 2000 mm (6' 6 3/4'') allow for

unusual floor plans

**Aesthetics**

Flush-fitting front panel with a uniform gap pattern

**Technical guidelines** Door weight limit

Door height limit Door width limit Door weight Door thickness Door height Door width

Max.

Max. Max.

40 kg (88 lbs.)

19–25 mm (3/4'' to 31/32'')

2600 mm (8' 6 3/8'')

900 mm (2' 11 7/16'')

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

40 F IS

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Aperto 40 F IS consisting of running track incl. curve for parking area (aluminum wall thickness 2.8 mm (1/8'')) 2-piece, suspension brackets, running gear with ball bearing rollers, fixing cup with hanger bolt, spacers for door gaps, end buffer, bottom guide pin, bottom guide profile

Optional:

(….) Center stop

(….) Straightening fitting

# Interfaces Door leaf

* Top, drill hole at rear for suspension
* Suspension cup with screw fixing

- Door thickness 19–25 mm (3/4'' to 31/32'')

* Bottom guide part, screwed on at rear

# Parking area

- Up to 7 sliding door elements

# Hawa Sliding Solutions AG

Untere Fischbachstrasse 4, 8932 Mettmenstetten, Switzerland

Phone +41 44 787 17 17, [info@hawa.com,](mailto:info@hawa.com) [www.hawa.com](http://www.hawa.com/) 1