**Fitting for top-running glass doors up to 60 kg (132 lbs.), with surface mounted running track.**

**Ceiling mounting. Fully opening.**

**Product-Highlights**

**Aesthetics**

Small installation dimensions and narrow glass retaining profiles

**Flexibility**

Also suitable for outdoor use in an inland climate

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

60 kg (132 lbs.)

8–10 mm (5/16'' to 13/32'')

2600 mm (8' 6 3/8'')

1100 mm (3' 7 5/16'')

10900 mm (35' 9 1/8'')

+/- 3 mm (1/8'') No

Glass

Aluminum raw;Aluminum anodized / aluminum stainless steel effect

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** External blinds and shutters - Resistance to wind loads - Method of testing EN 1932 (03/2003)

* Class 5 wind resistance

Operating forces - Test method - Part: Windows EN 12046-1 (11/2003)

* Class 2 operating force

Shutters EN 13659 (06/2004) + A1 (10/2008)

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Aperto 60 GL consisting of running track incl. curve for parking area (aluminum wall thickness 2.8 mm (1/8'')) 2-piece, suspension brackets, running gear with ball bearing rollers, suspension and glass retaining profile with cover panel, suspension carriage

Optional:

( ) Bottom guide profile

( ) Rotary handle

( ) Cylinder modules

( ) Protective edge trim

# Interfaces Door leaf

* Glass processing for glass holders

# Parking area

* Parking area parallel to sliding axis or at 90° to sliding axis
* Concealed parking area behind hinged door or visibly parked cabinet fronts as design element
* An additional hinged door set must be ordered with a concealed parking area behind a hinged door