

**Fitting for top-running wooden doors up to 60 kg (132 lbs.), with surface mounted running**

**track. Ceiling mounting. Fully opening.**

**Product-Highlights**

**Aesthetics**

Specially developed for light partition walls up to 60 kg (132 lbs.),

allowing for visible parts with smaller dimensions

**Productivity** Order the entire system with three to four article numbers

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

60 kg (132 lbs.)

35–50 mm (1 3/8'' to 1 31/32'')

2600 mm (8' 6 3/8'')

1500 mm (4' 11 1/16'')

13600 mm (44' 7 7/16'')

+/- 3 mm (1/8'') No

Wood

Aluminum anodized

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Aperto 60 H consisting of running track incl. curve for parking area (aluminum wall thickness 2.8 mm (1/8'')) 2-piece, suspension brackets, running gear with ball bearing rollers, suspension profile with suspension carriage,

Optional:

( ) Sealing profile

( ) Protective edge trim

( ) Bottom guide

( ) Bottom guide profile

( ) Bar bolt lock

( ) Rotary handle

# Interfaces Door leaf

* Recess for suspension profile (H × W) 25 × 20 mm (31/32'' x 25/32'')
* Screwed-on suspension profiles
* Recess for bottom guide part (H × W) 25 × 20 mm (31/32'' x 25/32'') (optional)

# Parking area

* Parking area parallel to sliding axis or at 90° to sliding axis
* Concealed parking area behind hinged door or visibly parked cabinet fronts as a design elemen
* An additional hinged door set must be ordered with concealed parking area behind a hinged door