

**Fitting for top-running glass doors up to 40 kg (88 lbs.), with surface mounted running track.**

**With soft and self closing mechanism. Wall mounting. Niche solution.**

**Product-Highlights**

**Productivity** Simple connection technology between the individual components

makes quick installation possible

**Flexibility**

Different fixing methods make applications with wall-wall, glass-wall,

or glass-glass combinations possible

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

40 kg (88 lbs.)

8/10 mm (5/16'' to 13/32'')

2200 mm (7' 2 5/8'')

800 mm (2' 7 15/32'')

1500 mm (4' 11 1/16'')

+2 / -3 mm (+3/32'' / -1/8'')

Yes Glass

**System options**

Wall mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to DIN EN 1527 – Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Banio 40 GF consisting of running track (aluminum), clip-on panel, running gear with friction bearing rollers, damper, stopper, clamping shoe with hanger bolt, bottom guide, handle set, splash quard profile, Banio sealing set

Optional:

( ) partial threshold

# Interfaces Door leaf

* No recess
* Clamped glass fixing

# Glass wall

* Glass cut-out for corner connector