

**Fitting for top-running glass folding sliding walls up to 80 kg (176 lbs.), with surface mounted**

**running track or running track flush with the ceiling. Ceiling mounting.**

**Product-Highlights**

**Aesthetics**

Straight and rounded glass retaining profile for different design

requirements

**Flexibility**

Thanks to having identically designed profiles, it can be combined

with Hawa Variotec

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

80 kg (176 lbs.)

10–12.7 mm (13/32'' to 1/2'')

2600 mm (8' 6 3/8'')

900 mm (2' 11 7/16'')

6000 mm (19' 8 7/32'')

+/- 3 mm (1/8'') No

Glass

**System options**

Ceiling mounting

Ceiling mounting recessed Top-running

Yes

Yes Yes

**Application area**

Utilization medium / semi-public access

Utilization high / public access

Yes

Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 1998 – Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859 / 2004

* Overload test
* Function test

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Centerfold 80 GV consisting of running track (aluminum wall thickness 3.0 mm (1/8'')), running gear with ball bearing rollers, suspension carriage, suspension and glass retaining profiles, top pivot, hinges, end stop, Falt-und Drehtürschnäpper, bar bolt lock, floor sleeve

Optional:

(….) Guide track (….) Connecting rod

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing on suspension and glass retaining profiles