

**Fitting for top-running glass doors up to 100 kg (220 lbs.), with surface mounted running track.**

**Optionally with soft and self closing mechanism. Wall or ceiling mounting.**

**Product-Highlights**

**Flexibility**

Ceiling mounting with integrated clip-on panel in aluminum or wood

**Productivity** Multi-track guide and running tracks reduce installation cost

**Technical guidelines** Max. Door weight

Door thickness

Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

100 kg (220 lbs.)

30 mm (1 3/16'')

(5.9–10 mm (7/32'' to 13/32''))

2750 mm (9' 9/32'')

1200 mm (3' 11 1/4'')

6000 mm (19' 8 7/32'')

+/- 3 mm (1/8'') Yes

Alu Glass Wood Mix Aluminum anodized

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 1998

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Overload test
* Function test

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 100 GR consisting of running track (aluminum), clip-on panel, running gear with ball bearing rollers and running gear support, aluminum glass frame profile, stopper with retention spring, bottom guide

Optional:

( ) Multi-track running track

( ) Intermediate panel

( ) Frame bars

( ) Frame profile with vertical handle

(. ) Clip-on component for wooden and aluminum panel

(. ) Cover cap for assembly opening

(. ) Hawa Porta 100 soft and self closing mechanism

(. ) Wall compensation profile

# Interfaces Door leaf

* Screw fixed running gear support
* Profiles cut at right angles and screw fixed
* Customer-provided panel