**Fitting for top-running wooden doors up to 100 kg (220 lbs.), with surface mounted running**

**track. With soft and self closing mechanism. Ceiling mounting. Minimal installation height.**

**Product-Highlights**

**Flexibility**

Ceiling-integrated or surface-mounted installation with the same

system

**Productivity** Tool-less door mounting

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

100 kg (220 lbs.)

28–30 mm (1 3/32'' to 1 3/16'')

2400 mm (7' 10 7/16'')

1200 mm (3' 11 1/4'')

6000 mm (19' 8 7/32'')

+1 / -3 mm (+1/32'' / -1/8'')

Yes Wood

Aluminum anodized

**System options**

Wall mounting

Ceiling mounting

Ceiling mounting recessed

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 1998

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Overload test
* Function test

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Divido 100 HM consisting of running track (aluminum), running gear with ball bearing rollers, stopper with retention spring, plastic running gear carrier with steel housing, bottom guide with roller.

Optional:

( ) Multi-track running track

( ) Cover profile for double running track

( ) Hawa Porta 100 soft and self closing mechanism

( ) Cover cap for assembly opening

( ) Bottom guide set for wall mounting with roller

( ) Wall compensation profile

# Interfaces Door leaf

– Recess for housing (H × W) 23 × 18 mm (29/32'' × 23/32'')

* Screw fixing of the housing

– Guide groove (H × W) 16 × 12 mm (5/8'' × 15/32'')