Hardware for pivoting, folding and lateral sliding in of wooden doors up to 25 kg (55 lbs.). Uniform, flush front design with even gap pattern. Push-to-open function for handle-less cabinet designs.

**Product-Highlights Flexibility** Variable door dimensions, also for floor-to-ceiling, walk-in

closets – can be combined with Hawa Concepta III for three-door solutions without separating wall

**Productivity** Easy installation thanks to high degree of pre-assembly and intuitive adjustment

**Aesthetics** Cabinet designs without handle – the technology remains invisible

**Technical guidelines** Door weight 10–25 kg (22 to 55 lbs.)

Door thickness 18–26 mm (23/32'' to 1 1/32'')

Door height 1900–2700 mm (6' 2 13/16'' to 8' 10 5/16'')

Door width 440–750 mm (1' 5 5/16'' to 2' 5 17/32'')

Height adjustable +/- 3 mm (1/8'')

Door material Wood

Aluminum anodized /

Finish color of visible profiles

Aluminum black anodized

**Application area** Utilization light / semi-public access Yes

Utilization medium / semi-public access Yes

**Tests**

**Warranty**

**Product Design**

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts in accordance with DIN EN 15706 / 2009

Hardware for furniture – Strength and durability of hinges and their components – Hinges pivoting on a vertical axis in accordance with DIN EN 15570 / 20082008

With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

Hawa Folding Concepta III 25 Push consisting of running and guide profiles (aluminum),

a slide-in unit with door ejection cabinet connection profiles (Connector 110 mm (4 11/32'')), upright profile, concealed hinges, center concealed hinges spring loaded, slide-in securing mechanism, folding door soft closing mechanism, Push-to-open for folding door.

Optional:

( ) Base profile set

( ) Reinforcement profile

( ) Magnetic centering part

( ) Straightening fitting

**Interfaces Door leaf**

* 35 mm (1 3/8'') drill holes for concealed hinges
* 35 mm (1 3/8'') drill holes for center concealed hinges
* Drill holes for hardware components

**Cabinet side and outer side**

* Drill holes for hardware components

**Cabinet designs**

* Door striking against the top and bottom cabinet section
* Floor-to-ceiling doors
* Door with furniture plinth
* Door without furniture base