**Fitting for top-running wooden or metal shutters up to 60 kg (132 lbs.), with low running track.**

**Ceiling or architrave mounting.**

**Product-Highlights**

**Aesthetics**

Minimal rail height

**Security**

The shutters withstand even stormy winds, both open and closed

**Technical guidelines** Max. shutter weight

Shutter thickness Max. shutter height

Max. shutter widht

60 kg (132 lbs.)

≥28 mm (1 3/32'')

3200 mm (10' 5 31/32'')

400–3750 mm (1' 3 3/4'' to 12' 3 5/8'')

(Max. shutter area 9.6 m² (103 ft²))

max. attack surface per shutter

Max. system width Max. shading area Height adjustable

9.6 m²

7500 mm (24' 7 9/32'')

9.6 m²

+/- 2 mm (3/32'')

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Inland, more than 20 km from the coast

Yes

Yes Yes Yes

**Tests** Building hardware – hardware for sliding doors and in accordance with EN 13659 DIN EN 1670

* Resistance to wind load; class 6 in accordance with EN 13659
* Operating force: Class 1 in accordance with EN 13659

Furniture fittings – roller fittings for sliding doors in accordance with DIN EN 1670

* Corrosion resistance: Class 4 (very high resistance, external area with very harsh conditions)

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

# Place of use

Outdoor area with rural inland climate, without particularly high pollution level and at least 20 km from the sea.

**Product Design** Hawa Frontslide 60 A niedrig consisting of top running track (aluminum wall thickness 3.0 mm (1/8'')), running track with plastic rollers, track buffer with adjustable retention, bottom guide track and guide component.

Optional:

( ) Mehrbahnig möglich

(….) Befestigung oben an Wand mit Winkel bauseits ( ) Fixed to wall or floor at bottom

( ) Sliding shutter stop

( ) Sliding shutter lock

( ) Sliding shutter arrester

# Interfaces Door leaf

* Screwed on or riveted from above
* Door thickness ≥28 mm (≥1 3/32'')
* Guide component screwed on at bottom