**Fitting for top-running glass doors up to 100 kg (220 lbs.), with running track flush with the ceiling. Optionally with soft and self closing mechanism. Wall or ceiling mounting. Minimal installation height.**

**Product-Highlights Comfort** Accessible opening and soft and self closing at both sides from door

widths of 800 mm (2' 7 1/2")

**Flexibility** Running tracks for wall and ceiling mounting with integrated clip-on system

**Security** Performance guarantee: 15 years for private use and 7 years for commercial use on incomparably low opening forces of max. 22 N

**Technical guidelines** Max. Door weight 100 kg (220 lbs.)

Door thickness 8–12.7 mm (5/16'' to 1/2'')

Max. Door height 4000 mm (13' 1 15/32'')

Max. Door width 3000 mm (9' 10 1/8'')

Max. Opening width 2950 mm (9' 8 5/32'')

Height adjustable +/- 3 mm (1/8'')

Soft close Yes

Guaranteed opening force with damping\* Max. 22 N (fully accessible) Door material Glass

Finish color of visible profiles Aluminum anodized / aluminum stainless steel effect

**System options** Wall mounting Yes

Ceiling mounting Yes

Ceiling mounting recessed Yes

Top-running Yes

**Application area** Utilization light / semi-public access Yes

Utilization medium / semi-public access Yes

Utilization high / public access Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

\*see warranty

**Warranty** Performance guarantee for all official Hawa Junior 100 versions with magnetic soft close system: Guaranteed opening force of the sliding doors of max. 22 N for 15 years in domestic use and 7 years in commercial use

The performance guarantee is valid worldwide with the exception of contractual partners with their registered office/residence in the USA and use of the products by end users with registered office/residence in the USA.

Additional function guarantee on all parts other than those subject to wear and tear: 2 years

**Product Design** Hawa Junior 100 GP consisting of running track (aluminum wall thickness 2.9 mm (1/8'')), running gear with friction bearing rollers, stopper or soft closing mechanism Hawa SoftMove 100, glass suspension with point fixing, bottom guide with zero clearance

Optional:

(….) Guide track

(….) Track set for fixed glazing

(….) Hawa Adapto 80 concrete casting system (….) Bottom door stopper, with centering part

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing with point fixing

# Hawa Adapto concrete casting system

* The Hawa Adapto 80 concrete casting system is already integrated in the concrete ceiling of the building shell