

**Fitting for top-running glass doors up to 120 kg (264 lbs.), with surface mounted running track**

**or running track flush with the ceiling. Optionally with soft and self closing mechanism. Wall or ceiling mounting.**

**Product-Highlights**

**Aesthetics**

Neutral, linear design

**Security**

Very safe thanks to positive-fit glass fixing

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

120 kg (264 lbs.)

8–16 mm (5/16'' to 5/8'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 3 mm (1/8'') Yes

Glass

**System options**

Wall mounting

Ceiling mounting

Ceiling mounting recessed Top-running

Yes

Yes Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 120 G consisting of running track (aluminum wall thickness 3.5 mm (5/32'')), running gear with friction bearing rollers, stopper or soft closing mechanism Hawa SoftMove 120, suspension profile with suspension carriage, bottom guide with zero clearance, suspension and glass retaining profiles

Optional:

(….) Guide track

(….) Running track set with fixed glazing (….) Angled profile for wall mounting ( ) Cover cap to angled profile

( ) Hawa Adapto concrete casting system 120

(….) Bar bolt lock

(….) Bottom door stopper, with centering part

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing on suspension and glass retaining profiles

# Hawa Adapto concrete casting system

* The Hawa Adapto 120 concrete casting system is already integrated in the concrete ceiling of the building shell