

**Fitting for top-running glass doors up to 160 kg (325 lbs.), with surface mounted running track**

**or running track flush with the ceiling. Ceiling mounting.**

**Product-Highlights**

**Aesthetics**

Neutral, linear design

**Security**

Very safe thanks to positive-fit glass fixing

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

160 kg (352 lbs.)

8–16 mm (5/16'' to 5/8'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 3 mm (1/8'') No

Glass

**System options**

Ceiling mounting

Ceiling mounting recessed Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 160 G consisting of running track (aluminum wall thickness 4.0 mm (5/32'')), running gear with friction bearing rollers, stopper, suspension profile with suspension carriage, bottom guide with zero clearance, suspension and glass retaining profiles

Optional:

( ) Guide track

( ) Track set for fixed glazing

( ) Bar bolt lock

( ) Bottom door stopper, with centering part

**Interfaces Door leaf**- Glass processing for glass holders

– Positive-fit glass fixing on suspension and glass retaining profiles