

**Fitting for top-running glass doors up to 160 kg (352 lbs.), with surface mounted running track**

**or running track flush with the ceiling. Ceiling mounting. Minimal installation height.**

**Product-Highlights**

**Aesthetics**

Cover caps in different design versions

**Productivity** Easy height adjustment via both suspensions on completely installed

door

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

160 kg (352 lbs.)

8–12.7 mm (5/16'' to 1/2'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 4 mm (5/32'')

No Glass

**System options**

Ceiling mounting

Ceiling mounting recessed Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013 – Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 160 GP consisting of running track (aluminum wall thickness 4.0 mm (5/32'')), running gear with friction bearing rollers, stopper, Glass suspension with point fixing, suspension profile with suspension carriage, bottom guide with zero clearance

Optional:

( ) Guide tracks

( ) Bottom door stopper, with centering par

( ) Connector parts to profiles

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing with point fixing