# Tests



**Fitting for top-running glass doors up to 250 kg (551 lbs.), with surface mounted running track**

**or running track flush with the ceiling. Ceiling mounting.**

**Product-Highlights**

**Comfort**

High quality steel ball bearing rollers for quiet, smooth running, even

with heavy weights

**Security**

Very safe thanks to positive-fit glass fixing

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

250 kg (551 lbs.)

8–16 mm (5/16'' to 5/8'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 5 mm (3/16'')

No Glass

**System options**

Ceiling mounting

Ceiling mounting recessed Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Warranty**

Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 250 G consisting of running track (aluminum wall thickness 4.5 mm (3/16'')), running gear with friction bearing rollers, stopper, suspension profile with suspension carriage, bottom guide with zero clearance, suspension and glass retaining profiles

Optional:

( ) Guide track

( ) Bar bolt lock

( ) Bottom door stopper, with centering part

( ) Connector parts to profiles

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing on suspension and glass retaining profiles