

Fitting for top-running wooden doors up to 40 kg (88 lbs.), with surface mounted running track or running track flush with the ceiling. Optionally with soft and self closing mechanism. Ceiling mounting. Minimal installation height. Wall pocket solution.

**Product-Highlights Flexibility** The running track can be installed and removed at any time

**Aesthetics** Thanks to integrated spring stop with Push-to-open function, there are no visible hardware components, door milling grooves or spring handles at the edge of the door

**Technical guidelines** Max. Door weight 40 kg (88 lbs.)

Door thickness 35–80 mm (1 3/8'' to 3 5/32'')

Max. Door height 4000 mm (13' 1 15/32'')

Max. Door width 1250 mm (4' 1 7/32'')

Max. Opening width 1220 mm (4' 1/32'')

Height adjustable +/- 3 mm (1/8'')

Soft close Optional

Door material Wood

**System options** Ceiling mounting Yes

Ceiling mounting recessed Yes

Top-running Yes

**Application area** Utilization light / semi-public access Yes

Utilization medium / semi-public access Yes

Utilization high / public access Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013 – Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 40 B Pocket consisting of running track (aluminum wall thickness 2.0 mm (3/ 32'')), running gear with friction bearing rollers, stopper, spring buffer or soft closing mechanism Hawa SoftMove 40, suspension profile with suspension carriage, bottom guide with zero clearance

Optional:

( ) Guide track, for groove mounting, plastic

( ) Set for installable and removable running track

# Interfaces Door leaf

* Recess for suspension profile (H × B) 25 × 20 mm (31/32'' × 25/32'')
* Screw fixing of the suspension profiles
* Guide groove (H × B) 20 × 10 mm (25/32'' × 13/32'') (20 × 12 mm (25/32'' × 13/32'') with plastic guide track)

# Pocket construction

* Pocket construction must be taken care of by the customer

# Assembly set

* The retainer profile is installed during the creation of the pocket construction