

**Fitting for 2 symmetrically opening glass doors up to 80 kg (176 lbs.), with surface mounted**

**running track or running track flush with the ceiling. Ceiling mounting.**

**Product-Highlights**

**Flexibility**

Door openings up to 2280 mm (7' 5 3/4 '')

**Aesthetics**

Symmetrical solution without guide track possible

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Door width

Max. Opening width Height adjustable Soft close

Door material

80 kg (176 lbs.)

8–16 mm (5/16'' to 5/8'')

3000 mm (9' 10 1/8'')

500–1200 mm (1' 7 11/16'' to 3' 11 1/4'')

2300 mm (7' 6 9/16'')

+/- 3 mm (1/8'') No

Glass

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 80 G Symmetric consisting of running track (aluminum wall thickness 2.9 mm (1/8'')), running gear with friction bearing rollers, stopper, toothed belt with deflection rollers, suspension profile with suspension carriage, bottom guide with zero clearance, suspension and glass retaining profiles

Optional:

( ) Guide track

( ) Bottom door stopper, with centering part

**Interfaces Door leaf**- Glass processing for glass holders

– Positive-fit glass fixing on suspension and glass retaining profiles