

**Fitting for 2 telescopic opening glass doors up to 80 kg (176 Ibs.), with surface mounted**

**running track. Ceiling mounting.**

**Product-Highlights**

**Flexibility**

Door openings up to 3000 mm (9'10 1/8'') wide

**Flexibility**

Telescopic opening without guide track

**Technical guidelines** Max. Door weight

Door thickness

Max. Door height Door width

Max. Opening width Height adjustable Soft close

Door material

80 kg (176 lbs.)

8–16 mm (5/16'' to 5/8'')<br>(Fully tempered monolithic glass (ESG)) 2600 mm (8' 6 3/8'')

500–1000 mm (1' 7 11/16'' to 3' 3 3/8'')

3700 mm (12' 1 21/32'')

+/- 2 mm (3/32'')

No Glass

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013 – Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 80 G Telescopic consisting of running track (aluminum wall thickness 2.9 mm (1/ 8'')), running gear with friction bearing rollers, stopper, toothed belt with deflection rollers, suspension profile with suspension carriage, bottom guide with zero clearance, suspension and glass retaining profiles

Optional:

(….) Guide track

(….) Running track set with fixed glazing

(….) Bottom door stopper, with centering part

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing on suspension and glass retaining profiles