**Fitting for top-running wooden doors up to 80 kg (176 lbs.), with surface mounted running**

**track. Ceiling mounting. Outdoor version.**

**Product-Highlights**

**Comfort**

Rollers made from high-performance plastic are the guarantee of quiet

running and easy sliding

**Security**

Corrosion-resistant materials for use in interior rooms which are

temporarily damp

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

80 kg (176 lbs.)

35–80 mm (1 3/8'' to 3 5/32'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 4 mm (5/32'')

No Wood

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 80 Inox consisting of running track (aluminum wall thickness 2.9 mm

(1/8'')), running gear with friction bearing rollers, stopper, Hanger bracket, bottom guide with zero clearance

Optional:

( ) Guide track, for groove mounting, plastic

**Interfaces Door leaf**

– Screw fixing of the hanger bracket

– Guide groove (H × W) 20 × 10 mm (25/32'' × 13/32'') (20 × 12 mm (25/32'' × 15/32'') with plastic guide track)