**Fitting for top-running metal doors up to 80 kg (176 lbs.), with surface mounted running track**

**or running track flush with the ceiling. Optionally with soft closing mechanism. Wall or ceiling mounting.**

**Product-Highlights**

**Aesthetics**

Neutral, linear design

**Security**

Very safe thanks to positive-fit glass fixing in metal door frame

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

80 kg (176 lbs.)

35–80 mm (1 3/8'' to 3 5/32'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 4 mm (5/32'')

Yes Metal

**System options**

Wall mounting

Ceiling mounting Top-running

Yes

Yes Yes

**Application area**

Utilization medium / semi-public access

Utilization high / public access

Yes

Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 80 M consisting of running track (aluminum wall thickness 2.9 mm

(1/8'')), running gear with friction bearing rollers, stopper or soft closing mechanism Hawa SoftMove 80, hanger bracket, bottom guide.

Optional:

( ) Guide track

( ) Bottom door stopper, with centering part

# Interfaces Door leaf

– Screw fixing of the hanger bracket