

Fitting for top-running wooden doors up to 80 kg (176 lbs.), with surface mounted running track. Optionally with soft and self closing mechanism. Ceiling mounting. Wall pocket solution.

**Product-Highlights Flexibility** The running track can be installed and removed at any time

**Aesthetics** Thanks to integrated spring stop with Push-to-open function, there are no visible hardware components, door milling grooves or spring handles at the edge of the door

**Technical guidelines** Max. Door weight 80 kg (176 lbs.)

Door thickness 35–80 mm (1 3/8'' to 3 5/32'')

Max. Door height 4000 mm (13'1 15/32'')

Max. Door width 1500 mm (4'11 1/16'')

Max. Opening width 1470 mm(4' 9 7/8'')

Height adjustable +/- 4 mm (5/32'')

Soft close Yes

Door material Wood

Finish color of visible profiles Aluminum anodized

**System options** Ceiling mounting Yes

Top-running Yes

**Application area** Utilization light / semi-public access Yes

Utilization medium / semi-public access Yes

Utilization high / public access Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 /2013 – Duration of functionality: Class 6\* (highest class = 100,000 cycles)

\* System without soft closing system has been tested with 200,000 cycles

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 80 B Pocket consisting of running track (aluminum wall thickness 2.9 mm (1/8'')), running gear with friction bearing rollers, stopper, spring buffer or soft closing mechanism Hawa SoftMove 80, two-way suspension, bottom guide with zero clearance

Optional:

( ) Guide track, for groove mounting, plastic

( ) Set for installable and removable running track

( ) Clip-on panel for retainer profile, for lintel panelling, aluminum

# Interfaces Door leaf

* Screw fixing of the two-way suspension
* Guide groove (H × B) 20 × 10 mm (25/32'' × 13/32'') (20 × 12 mm (25/32'' × 15/32'') with plastic guide track)

# Pocket construction

* Pocket construction must be taken care of by the customer

# Assembly set

* The retainer profile is installed during the creation of the pocket construction