**Fitting for 3 telescopic opening wooden doors up to 80 kg (176 lbs.), with surface mounted**

**running track. Ceiling mounting.**

**Product-Highlights**

**Flexibility**

Door openings up to 3200 mm (10' 5 31/32'') possible

**Flexibility**

Combination of telescopic and symmetrical opening possible

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Door width

Max. Opening width Height adjustable Soft close

Door material

80 kg (176 lbs.)

32–47 mm (1 1/4'' to 1 27/32'')

4000 mm (13' 1 15/32'')

500–1200 mm (1' 7 11/16'' to 3' 11 1/4'')

6750 mm (22' 1 3/4'')

+/- 2 mm (3/32'')

No Wood

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 2013

– Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Strength and durability of slide fittings for sliding doors and roll fronts according to EN 15706 / 2009

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Junior 80 Z Telescopic 3 consisting of running track (aluminum wall thickness 2.9 mm (1/8'')), running gear with friction bearing rollers, stopper, toothed belt with deflection rollers, two-way suspension, bottom guide with zero clearance

Optional:

( ) Guide track, for groove mounting, plastic

( ) Bottom door stopper, with centering part

# Interfaces Door leaf

– Screw fixing of the two-way suspension

– Guide groove (H × B) 25 × 10 mm (31/32'' × 13/32'') (20 × 12 mm (25/32'' × 15/32'') with plastic guide track)