**Fitting for top-running wooden or glass doors up to 70 kg (154 lbs.), with surface mounted**

**running track or guide track flush with the ceiling. Ceiling mounting.**

**Product-Highlights**

**Comfort**

Sprung bottom guide on continuous guide track for stable and quiet

sliding characteristics

**Aesthetics**

Filigree running track and minimal installation height for sophisticated

design requirements

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

70 kg (154 lbs.)

30–40 mm (1 3/16'' to 1 9/16'')

2600 mm (8' 6 3/8'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 3 mm (1/8'') No

Wood;Glass;Wood Glass Mix Aluminum raw;Aluminum anodized / aluminum stainless steel effect

**System options**

Ceiling mounting

Ceiling mounting recessed Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access

Yes

Yes

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Ordena 70 F consisting of running track, running gear with ball bearing rollers, suspension profile for wood or point fixing for glass, track buffer with retention spring, spring- loaded bottom guide, guide track

Optional:

( ) Double running track

( ) Double guide track

( ) Cover caps

( ) Wall connection profile

( ) Edge protection

# Interfaces Wooden door leaf

– Recess for housing (H × W) 25 × 20 mm (31/32'' x 25/32'')

* Screwed-on housing
* Drilled-in bottom guide Ø 12 mm (15/32'')

# Glass door leaf

* Glass processing for glass holder at top and bottom