**Fitting for 2 synchronously opening glass doors up to 100 kg (220 lbs.), with surface mounted**

**running track. Wall or ceiling mounting. With fixed glass support profile.**

**Product-Highlights**

**Flexibility**

Standard applications can be extended with the Synchro option

**Comfort**

Two simultaneously sliding doors make large, fully accessible

openings possible

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

100 kg (220 lbs.)

8–12.7 mm (5/16'' to 1/2'')

2700 mm (8' 10 5/16'')

1200 mm (3' 11 1/4'')

2300 mm (7' 6 9/16'')

+/- 4 mm (5/32'')

No Glass

**System options**

Wall mounting

Ceiling mounting Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to DIN EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Porta 100 GF Synchro consisting of running track with fixed glass profile (aluminum), clip-on, running gear with ball bearing rollers, stopper with retention spring, kevlar rope with deflection rollers, clamping shoe with hanger bolt, bottom guide with zero clearance,

Optional:

( ) Hawa Porta 100 soft and self closing mechanism

( ) Bottom door stopper, with centering part

# Interfaces Door leaf

* No recess
* Clamped glass fixing