

**Fitting for top-running wooden doors up to 100 kg (220 lbs.), with surface mounted running**

**track. Optionally with soft and self closing mechanism. Wall or ceiling mounting.**

**Product-Highlights**

**Flexibility**

Ceiling mounting with customer-provided panelling or integrated

clip-on panel in aluminium or wood

**Productivity** Retrofitting of all components through the provided assembly opening,

prevents contamination during construction work

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

100 kg (220 lbs.)

30–80 mm (1 3/16'' to 3 5/32'')

2700 mm (8'10 5/16'')

1600 mm (5'3'')

1535 mm (5' 7/16'')

+/– 3 mm (1/8'') Yes

Wood

Aluminum / aluminum anodized / aluminum black anodized

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to DIN EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Porta 100 H consisting of running track, running gear with ball bearing rollers, stopper with retention spring, support flange, bottom guide with roller

Optional:

(….) Hawa Porta 60/100 assembly set (….) Clip-on panel, aluminum

(….) Clip-on component, for wooden and aluminum panel (….) Hawa Porta 100 soft and self closing mechanism (….) Cover cap for assembly opening

(….) Bracket for wall mounting

(….) Bottom guide set for wall mounting, with roller

**Interfaces Door leaf**

* Screw fixing of the support flange

– Guide groove (H × W) 16 × 12 mm (5/8'' × 15/32'')