

**Fitting for 2 synchronously opening wooden doors up to 100 kg (220 lbs.), with surface**

**mounted running track. Wall or ceiling mounting.**

**Product-Highlights**

**Flexibility**

Standard applications can be extended with the Synchro option

**Comfort**

Two doors open simultaneously and make large openings possible

**Aesthetics**

Also available in black as a “Black Edition” design option for a

particularly attractive appearance

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

100 kg (220 lbs.)

30–80 mm (1 3/16'' to 3 5/32'')

2700 mm (8' 10 5/16'')

1200 mm (3' 11 1/4'')

2300 mm (7' 6 9/16'')

+/- 3 mm (1/8'') No

Wood

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to DIN EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Porta 100 H Synchro consisting of running track (aluminum), clip-on panel, running gear with ball bearing rollers, stopper with retention spring, kevlar rope with deflection rollers, support flange, bottom guide with roller

Optional:

( ) Hawa Porta 60/100 assembly set

( ) Clip-on component, for wooden and aluminum panel

# Interfaces Door leaf

* Screw fixing of the support flange

– Guide groove (H × W) 16 × 12 mm (5/8'' × 15/32'')