

**Fitting for top-running glass doors up to 40 kg (88 lbs.), with surface mounted running track.**

**Glass panel installation.**

**Product-Highlights**

**Flexibility**

Mounting on solid walls or glass walls with optional glass wall adapters

**Productivity** No glass processing thanks to clamping shoe connection

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

40 kg (88 lbs.)

8 mm (5/16'')

2200 mm (7' 2 5/8'')

1000 mm (3' 3 3/8'')

950 mm (3' 1 13/32'')

+4/-1 (+5/32''/-1/32'')

Yes Glass

Aluminum anodized / aluminum stainless steel effect

**System options**

Wall mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access

Yes

Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

# **Product Design** Hawa Porta 40 GE Glass panel installation consisting of running track with glass wall mounting set (aluminum), clip-on panel, running gear with ball bearing rollers, stopper, clamping shoe with hanger bolt, bottom guide

Optional:

(….) Hawa Porta 40 soft and self closing mechanism

**Interfaces Door leaf**

* Recess for support holder
* Clamped glass fixing