

**Fitting for top-running wooden doors up to 40 kg (88 lbs.), with surface mounted running**

**track. Optionally with soft and self closing mechanism. Wall mounting.**

**Product-Highlights**

**Flexibility**

Multi-faceted product range, same parts for wooden and glass

solutions

**Productivity** No door processing, continuous adjustment for minimal production

times

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

40 kg (88 lbs.)

18–30 mm (23/32'' to 1 3/16'')

2200 mm (7' 2 5/8'')

1000 mm (3' 3 3/8'')

950 mm (3' 1 13/32'')

+2/-1 mm (+3/32''/-1/32'')

Yes Wood

Aluminum anodized / aluminum stainless steel effect

**System options**

Wall mounting

Top-running

Yes

Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access

Yes

Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

# **Product Design** Hawa Porta 40 H consisting of running track (aluminum), clip-on panel, running gear with friction bearing rollers, stopper, support flange, bottom guide

Optional:

(….) Spacer track

Hawa Porta 40 soft and self closing mechanism

**Interfaces Door leaf**

* Screw fixing of the support flange