**Fitting for top-running wooden doors up to 45 kg (99 lbs.), with surface mounted running**

**track. Wall or ceiling mounting.**

**Product-Highlights**

**Flexibility**

Wall and ceiling mounting to the same system with accessories

**Productivity** Easy processing for minimal production and installation times

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

45 kg (99 lbs.)

30–45 mm (1 3/16'' to 1 25/32'')

2200 mm (7' 2 5/8'')

1000 mm (3' 3 3/8'')

950 mm (3' 1 13/32'')

+/- 3 mm (1/8'') No

Wood

Aluminum anodized

**System options**

Wall mounting

Ceiling mounting Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access

Yes

Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

# **Product Design** Hawa Porta 45 H consisting of running track (aluminum), running gear with friction bearing rollers, stopper with retention spring, support flange, bottom guide

Optional:

(….) Bracket set for wall mounting

(….) Bottom guide set for wall mounting, with roller

**Interfaces Door leaf**

* Screw fixing of the support flange