**Fitting for top-running wooden doors up to 600 kg (1320 lbs.), with surface mounted running**

**track. Wall or ceiling mounting.**

**Product-Highlights**

**Flexibility**

Three or four point guidance for maximum stability

**Comfort**

Even heavy doors close smoothly and quietly thanks to the ball

bearing rollers

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

600 kg (1320 lbs.)

40–100 mm (1 9/16'' to 3 15/16'')

6000 mm (19' 8 7/32'')

5000 mm (16' 4 27/32'')

4950 mm (16' 2 7/8'')

+10 / -5 mm (+13/32'' / -3/16'')

No Wood

**System options**

Wall mounting

Ceiling mounting Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to DIN EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Porta 600 H consisting of running track (steel), running gear with ball bearing rollers, stopper with rubber buffer, support flange, bottom door stopper

Optional:

( ) Guide track steel

( ) Support bracket for bottom guide

( ) Track connection

# Interfaces Door leaf

* Screw fixed or welded attachment of the support flange

– Guide groove (H × W) 25 × 7 mm (31/32'' × 9/32'') (25 × 25 mm (31/32'' × 31/32'') with steel guide track)