**Fitting for top-running wooden doors up to 60 kg (132 lbs.), with surface mounted running track. Optionally with soft and self closing mechanism. Wall mounting.**

**Product-Highlights Flexibility** Wall mounting with integrated clip-on panelling in wood or aluminium with stylish end pieces

**Productivity** Retrofitting of all components through the provided assembly opening, prevents contamination during construction

**Aesthetics** Also available in black as a “Black Edition” design option for a particularly attractive appearance

**Technical guidelines** Max. Door weight 60 kg (132 lbs.)

Door thickness 30–45 mm (1 3/16'' to 1 25/32'')

Max. Door height 2700 mm (8' 10 5/16'')

Max. Door width 1600 mm (5' 3'')

Max. Opening width 1535 mm (5' 7/16'')

Height adjustable +/– 3 mm (1/8'')

Soft close Yes

Door material Wood

Finish color of visible profiles Aluminum / aluminum anodized / aluminum black anodized

**System options** Wall mounting Yes

Top-running Yes

**Application area** Utilization light / semi-public access Yes

Utilization medium / semi-public access Yes

Utilization high / public access Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527

* Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Stop reliability
* Retention reliability

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Porta 60 HC consisting of running track, running gear with friction bearing rollers, stopper with retention spring, support flange, bottom guide with roller

Optional:

(….) Running track with extended spacing of +9 mm/+20 mm (+11/32''/+25/32'') (….) Clip-on panel, aluminum

(….) Clip-on component, for wooden and aluminum panel (….) Hawa Porta 60 soft and self closing mechanism

(….) Cover cap for assembly opening

(….) Bottom guide set for wall mounting, with roller

# Interfaces Door leaf

* Screw fixing of the support flange

– Guide groove (H × W) 16 × 12 mm (5/8'' × 15/32'')