**Fitting for 1 top-running glass door up to 80 kg (176 lbs.), with surface mounted running track or running track flush with the ceiling. With soft and self closing mechanism. Wall or ceiling mounting.**

**Product-Highlights Productivity** Suspension wedges accessible from below at any time for extremely

quick and easy door mounting and height adjustment

**Aesthetics** Technology integrated in the running track makes all-glass solutions possible without visible fitting parts.

**Technical guidelines** Max. Door weight 80 kg (176 lbs.)

Door thickness 8–12.7 mm (5/16'' to 1/2'')

Max. Door height 3000 mm (9' 10 1/8'')

Max. Door width 3000 mm (9' 10 1/8'')

Max. opening width 2900 mm (9' 6 3/16'')

Height adjustable +/- 3 mm (1/8'')

Soft close Yes

Door material Glass

Finish color of visible profiles Aluminum anodized;Aluminum anodized

/ aluminum stainless steel effect

**System options** Wall mounting Yes

Ceiling mounting Yes

Ceiling mounting recessed Yes

Top-running Yes

**Application area** Utilization light / semi-public access Yes

Utilization medium / semi-public access Yes

Utilization high / public access Yes

**Tests** Building hardware - Hardware for sliding doors and folding doors according to EN 1527/ 2013

– Duration of functionality and overloading class 3 = 100,000 cycles EN 15706: 2008 Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Purolino Plus 80 consisting of running track (aluminum), panel, running gear with ball bearing rollers, suspension wedge, soft closing mechanism, track buffer, floor guide with zero clearance

Optional:

(….) Profile set for fixed glazing

(….) Floor / wall connection profile for fixed glazing (….) Wall mounting system end profile set

(….) Wall mounting system wall profile set (….) Wall connection profile

(….) Protective edge trim (….) Vertical sealing profile (….) Bottom door stopper (….) Toplock lock

**Interfaces Door leaf**

– Glass processing for suspension wedge