

**Fitting for top-running glass doors up to 400 kg (882 lbs.), with surface mounted running track.**

**Ceiling mounting.**

**Product-Highlights**

**Security**

ESG up to 16 mm (5/8'') thick can be installed for greater stability of

the doors, especially with large elements

**Flexibility**

With weights of up to 400 kg (882 lbs.) per element, even unusual

building projects can be accomplished

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. opening width Height adjustable Soft close

Door material

Finish color of visible profiles

400 kg (882 lbs.)

8–16 mm (5/16'' to 5/8'')

3500 mm (11' 5 25/32'')

3000 mm (9' 10 1/8'')

12000 mm (39' 4 7/16'')

+/- 6 mm (1/4'') No

Glass;Alu Glass Wood Mix;Metal Aluminum anodized;Aluminum raw

**System options**

Ceiling mounting

Top-running

Yes

Yes

**Application area**

Utilization medium / semi-public access

Utilization high / public access

Yes

Yes

400 G

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Shopfront G 400 consisting of running track (stainless steel), running track with steel roller ball bearing, suspension and glass retaining profile, top pivot bearing, bottom guide piece, floor guide profile.

Optional:

(….) Bottom thrust bearing (….) Floor sleeve

(….) Bar bolt lock

# Interfaces Door leaf

* Glass with processing VSG/ ESG
* Positive-fitting glass fixing with point fixing
* Top and bottom profile sealed in with silicone

**Hawa Sliding Solutions AG**

Untere Fischbachstrasse 4, 8932 Mettmenstetten, Switzerland

Phone +41 44 787 17 17, [info@hawa.com,](mailto:info@hawa.com) [www.hawa.com](http://www.hawa.com/) 1