250 G

# Warranty

**Product Design**

With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

Hawa Super 250 G consisting of running track (stainless steel, wall thickness 5.0 mm (3/16'')), 3-roller running gear with ball bearing rollers, track buffer, suspension carriage, bottom guide with zero clearance, suspension and glass retaining profiles.

Optional:

(….) Edge protection

(….) Bottom glass retaining profile ( ) Bottom guide profile

(….) Bottom door stopper (….) Bar bolt lock



**Fitting for top-running glass doors up to 250 kg (551 lbs.), with surface mounted running track.**

**Wall or ceiling mounting.**

**Product-Highlights**

**Comfort**

High quality steel ball bearing rollers for quiet, smooth running, even

with heavy weights

**Security**

Very safe thanks to positive-fit glass fixing

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

250 kg (551 lbs.)

8–16 mm (5/16'' to 5/8'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 6 mm (1/4'') No

Glass;Alu Glass Wood Mix

Aluminum anodized / aluminum stainless steel effect

**System options**

Wall mounting

Ceiling mounting Top-running

Yes

Yes Yes

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Utilization high / public access

Yes

Yes Yes

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing on suspension and glass retaining profiles

# Hawa Sliding Solutions AG

Untere Fischbachstrasse 4, 8932 Mettmenstetten, Switzerland

Phone +41 44 787 17 17, [info@hawa.com,](mailto:info@hawa.com) [www.hawa.com](http://www.hawa.com/) 1