500 M

# Warranty

**Product Design**

With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

Hawa Super 500 M consisting of running track (stainless steel, wall thickness 5.0 mm (3/16'')), 3-roller running gear with ball bearing rollers, spring buffer, bottom guide.

Optional:

( ) Bottom guide profile

( ) Track stopper for screw fixing

**Fitting for top-running glass doors up to 500 kg (1102 lbs.), with surface mounted running**

**track. Wall or ceiling mounting.**

**Product-Highlights**

**Comfort**

High quality steel ball bearing rollers for quiet, smooth running, even with heavy weights

**Security**

Very safe thanks to positive-fit glass fixing

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

Finish color of visible profiles

500 kg (1102 lbs.)

35–80 mm (1 3/8'' to 3 5/32'')

4000 mm (13' 1 15/32'')

3000 mm (9' 10 1/8'')

2950 mm (9' 8 5/32'')

+/- 6 mm (1/4'') No

Alu Glass Wood Mix; Metal

Stainless steel

**System options**

Wall mounting

Ceiling mounting Top-running

Yes

Yes Yes

**Application area**

Utilization medium / semi-public access

Utilization high / public access

Yes

Yes

**Interfaces Door leaf**

* Cut-out for bracket suspension
* Rear drill hole for spring buffer Ø 20 mm (25/32'') / depth 102 mm (4 1/32'')
* Screw fixed bracket housing

– Guide groove (H × W) 40 × 6 mm (1 9/16'' x 1/4'')

**Hawa Sliding Solutions AG**

Untere Fischbachstrasse 4, 8932 Mettmenstetten, Switzerland

Phone +41 44 787 17 17, info@hawa.com, [www.hawa.com](http://www.hawa.com/) 1