

**Fitting for top-running glass doors up to 80 kg (176 lbs.), with surface mounted running track**

**or running track flush with the ceiling. Ceiling mounting.**

**Product-Highlights**

**Productivity** Simplified planning and ordering, since all elements are the same width

and are provided with the same cut-outs

**Aesthetics**

Straight and rounded glass retaining profile for different design

requirements

**Technical guidelines** Max. Door weight

Door thickness Max. Door height Max. Door width Max. Opening width Height adjustable Soft close

Door material

80 kg (176 lbs.)

10–12.7 mm (13/32'' to 1/2'')

2600 mm (8' 6 3/8'')

900 mm (2' 11 7/16'')

6310 mm (20' 8 7/16'')

+/- 3 mm (1/8'') No

Glass

**System options**

Ceiling mounting

Ceiling mounting recessed Top-running

Yes

Yes Yes

**Application area**

Utilization medium / semi-public access

Utilization high / public access

Yes

Yes

**Tests** Building hardware – Hardware for sliding doors and folding doors according to EN 1527 / 1998 – Duration of functionality: Class 6 (highest class = 100,000 cycles)

Hardware for furniture – Roller fittings for sliding doors according to DIN 68859

* Overload test
* Function test

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Variofold 80 GV consisting of running track (aluminum wall thickness 3.0 mm (1/8'')), running gear with ball bearing rollers, suspension carriage, suspension and glass retaining profiles, top pivot, bottom follower, hinges, end stop, folding and pivot door catch, bar bolt lock, floor sleeve

Optional:

(….) Guide track (….) Connecting rod

# Interfaces Door leaf

* Glass processing for glass holders
* Positive-fit glass fixing on suspension and glass retaining profiles