**Fitting for 1 vertically sliding wooden window leaf up to 150 kg (330 lbs.), with lateral guide**

**tracks and counterweight. Design Inslide. Half opening.**

**Product-Highlights**

**Comfort**

No restriction to use of space, since the open window does not

protrude into the room

**Productivity** Low production cost, as the rebates of the frame timbers correspond

to the standard

**Technical guidelines** Max. shutter weight

Shutter thickness Max. shutter height Max. shutter widht

150 kg (330 lbs.)

85 mm (3 11/32'')

1200 mm (3' 11 1/4'')

3200 mm (10' 5 31/32'')

**Application area**

Utilization light / semi-public access

Utilization medium / semi-public access Inland, more than 20 km from the coast Coastal area, less than 20 km from the coast

Yes

Yes Yes Yes

150 H

**Warranty** With the exception of parts subject to wear and tear, Hawa warrants the flawless functioning of the products delivered by it, as well as the durability of all parts, for a period of 2 years commencing from the transfer of risk.

**Product Design** Hawa Vertical 150 consisting of guide tracks (plastic), guide brackets, pin lock, wire cable 4 mm (5/32''), rope support, pulley bracket, deflection rollers

**Interfaces Counterweight**

* Customer-provided

**Paneling**

* Lining customer-provided
* Provide cavity at side and top for counterweight and deflection rollers

**Hawa Sliding Solutions AG**

# Untere Fischbachstrasse 4, 8932 Mettmenstetten, Switzerland

Phone +41 44 787 17 17, info@hawa.com, [www.hawa.com](http://www.hawa.com/) 1